**牙科CAD/CAM系统专用高硬度雕刻蜡盘**

Machinable Wax Disc for dentistry CAD/CAM System

青岛同泰蜡业有限公司采用国际先进配方和进口原材料自主研发生产的牙科CAD/CAM系统专用高硬度雕刻蜡盘，及高硬度雕刻蜡块，完全替代进口产品；废料可回收再加工,大幅度降低加工成本；

The Machinable Wax Disc for dentistry CAD/CAM System that is independently developed and produced by Qingdao Totem Candle Industry Co., adopts internationally advanced formula and imported raw materials. The production can completely replace the imported same kind of products. The waste can be recyclable and reprocessing. Also, the production can help you make a significant reduction in processing costs.

特性指标：

* 硬度：邵氏45-55度
* 软化点：105℃
* 滴熔点：140℃
* 密度：0.89-0.95
* 韧性：中上
* 灰度：0.03%
* 规格：直径98、112 mm，厚度14、16、18、20 mm; 其他规格
* 应用：齿科CAD/CAM系统专用雕刻蜡盘、蜡型模齿冠桥、失蜡铸造、首饰雕刻用蜡。

**Wax Disc Characteristics:**

* Hardness: 45-55(Shore "D" Scale)
* Softening point: 105℃
* Drop Melting Point: 140℃
* Density: 0.89-0.95
* Gray: 0.03%
* Resilience: good
* Size:Diameter98、112mm,thickness14,16,18,20mm as request.
* Application:in dentistry CAD / CAM system,tooth model,coating,machinable wax.